AV3

Prevention: redundant sensors

* Application providers can register redundant sensors in ApplicationActivationDB, next to the regular sensors (possible tactic: ‘predictive model’)

Detection: heartbeats

* Zie 2a: combinatie gateway & connection manager
* Eventueel connection manager opsplitsen om intern de structuur logisch bij te houden: aparte component die missing heartbeats telt
* Restructure TopologyConsultor 🡪 TopologyManager: more clear. Can consult and manage topology (i.e. adjust)
* Restructure/rename TopologyManager (🡪 ..DBManager): this contains more than only the topology, also configuration and information about sensors
* Restructure Topology 🡪 …DB (contains all information regarding sensors
* Restructure PeripheralDB 🡪 PeripheralTypeDB

Resolution: